******************
Maintenance
******************

The coldhead requires replacement of moving parts when the performance of the detector is observed to degrade after 10000 hours of operation. Contact Single Quantum when the 10000 hours are reach to plan the maintenance.
